;
; SIS 900/7016 Fast Ethernet NetWare Server Driver Information File
;

; version of this file:
  VER:  1.15
  SYN:  1.00

DR SIS900 OPT
{
        DES:            $SIS7016_DESC
        HELP:           $SIS7016_HELP
        PAR:            2.00
        PROD:           'PCI.1039.7016.1039.7016.*',
                        'PCI.1039.0900.1039.0900.*',
                        'PCI.1039.0900.1039.FFFF.*',
                        'PCI.1039.0900.0E11.B15E.*',
                        'PCI.1039.0900.1014.FFFF.*',
                        'PCI.1039.0900.1014.01B2.*',    ;IBM at Matic
                        'PCI.1039.0900.1014.01BA.*',    ;IBM
                        'PCI.1039.0900.1014.01BB.*',    ;IBM at USI
                        'PCI.1039.0900.1014.01FB.*',    ;IBM at USI
                        'PCI.1039.0900.1014.0201.*',    ;IBM at USI
                        'PCI.1039.0900.1014.FFFF.*',    ;IBM
                        'PCI.1039.0900.1019.0101.*',    ;ECS
                        'PCI.1039.0900.1019.0102.*',    ;ECS
                        'PCI.1039.0900.1019.0103.*',    ;ECS
                        'PCI.1039.0900.1019.0104.*',    ;ECS
                        'PCI.1039.0900.1019.0105.*',    ;ECS
                        'PCI.1039.0900.1019.0106.*',    ;ECS
                        'PCI.1039.0900.1019.0107.*',    ;ECS
                        'PCI.1039.0900.1019.0108.*',    ;ECS
                        'PCI.1039.0900.1019.0109.*',    ;ECS
                        'PCI.1039.0900.1019.0110.*',    ;ECS
                        'PCI.1039.0900.1019.0111.*',    ;ECS
                        'PCI.1039.0900.1019.0112.*',    ;ECS
                        'PCI.1039.0900.1019.0113.*',    ;ECS
                        'PCI.1039.0900.1019.0114.*',    ;ECS
                        'PCI.1039.0900.1019.0115.*',    ;ECS
                        'PCI.1039.0900.1019.0116.*',    ;ECS
                        'PCI.1039.0900.1019.0117.*',    ;ECS
                        'PCI.1039.0900.1019.0118.*',    ;ECS
                        'PCI.1039.0900.1019.0119.*',    ;ECS
                        'PCI.1039.0900.1019.0120.*',    ;ECS
                        'PCI.1039.0900.1019.0165.*',    ;ECS
                        'PCI.1039.0900.1019.0166.*',    ;ECS
                        'PCI.1039.0900.1019.0522.*',    ;ECS
                        'PCI.1039.0900.1019.0528.*',    ;ECS
                        'PCI.1039.0900.1019.0541.*',    ;ECS
                        'PCI.1039.0900.1019.0542.*',    ;ECS
                        'PCI.1039.0900.1019.0560.*',    ;ECS
                        'PCI.1039.0900.1019.0572.*',    ;ECS
                        'PCI.1039.0900.1019.0700.*',    ;ECS
                        'PCI.1039.0900.1019.0702.*',    ;ECS
                        'PCI.1039.0900.1019.0830.*',    ;ECS
                        'PCI.1039.0900.1019.0970.*',    ;ECS
                        'PCI.1039.0900.1019.0973.*',    ;ECS
                        'PCI.1039.0900.1019.0982.*',    ;ECS
                        'PCI.1039.0900.1019.0992.*',    ;ECS
                        'PCI.1039.0900.1019.0995.*',    ;ECS
                        'PCI.1039.0900.1019.0999.*',    ;ECS
                        'PCI.1039.0900.1019.0A01.*',    ;ECS
                        'PCI.1039.0900.1019.0A08.*',    ;ECS
                        'PCI.1039.0900.1019.0A14.*',    ;ECS
                        'PCI.1039.0900.1019.0A37.*',    ;ECS
                        'PCI.1039.0900.1019.0A38.*',    ;ECS
                        'PCI.1039.0900.1019.0A39.*',    ;ECS
                        'PCI.1039.0900.1019.0A40.*',    ;ECS
                        'PCI.1039.0900.1019.0A41.*',    ;ECS
                        'PCI.1039.0900.1019.0A42.*',    ;ECS
                        'PCI.1039.0900.1019.0A43.*',    ;ECS
                        'PCI.1039.0900.1019.0A44.*',    ;ECS
                        'PCI.1039.0900.1019.0A45.*',    ;ECS
                        'PCI.1039.0900.1019.0A46.*',    ;ECS
                        'PCI.1039.0900.1019.0D04.*',    ;ECS
                        'PCI.1039.0900.1019.0F05.*',    ;ECS
                        'PCI.1039.0900.1019.0F12.*',    ;ECS
                        'PCI.1039.0900.1019.0F17.*',    ;ECS
                        'PCI.1039.0900.1019.6000.*',    ;ECS
                        'PCI.1039.0900.1019.6001.*',    ;ECS
                        'PCI.1039.0900.1019.6002.*',    ;ECS
                        'PCI.1039.0900.1019.6003.*',    ;ECS
                        'PCI.1039.0900.1019.6004.*',    ;ECS
                        'PCI.1039.0900.1019.6005.*',    ;ECS
                        'PCI.1039.0900.1019.6006.*',    ;ECS
                        'PCI.1039.0900.1019.6007.*',    ;ECS
                        'PCI.1039.0900.1019.6008.*',    ;ECS
                        'PCI.1039.0900.1019.6009.*',    ;ECS
                        'PCI.1039.0900.1019.6010.*',    ;ECS
                        'PCI.1039.0900.1019.6011.*',    ;ECS
                        'PCI.1039.0900.1019.6012.*',    ;ECS
                        'PCI.1039.0900.1019.6013.*',    ;ECS
                        'PCI.1039.0900.1019.6014.*',    ;ECS
                        'PCI.1039.0900.1019.6015.*',    ;ECS
                        'PCI.1039.0900.1019.6016.*',    ;ECS
                        'PCI.1039.0900.1019.6017.*',    ;ECS
                        'PCI.1039.0900.1019.6018.*',    ;ECS
                        'PCI.1039.0900.1019.6019.*',    ;ECS
                        'PCI.1039.0900.1019.6020.*',    ;ECS
                        'PCI.1039.0900.1019.6021.*',    ;ECS
                        'PCI.1039.0900.1019.6022.*',    ;ECS
                        'PCI.1039.0900.1019.6023.*',    ;ECS
                        'PCI.1039.0900.1019.6024.*',    ;ECS
                        'PCI.1039.0900.1019.6025.*',    ;ECS
                        'PCI.1039.0900.1019.6026.*',    ;ECS
                        'PCI.1039.0900.1019.6027.*',    ;ECS
                        'PCI.1039.0900.1019.6028.*',    ;ECS
                        'PCI.1039.0900.1019.6029.*',    ;ECS
                        'PCI.1039.0900.1019.6030.*',    ;ECS
                        'PCI.1039.0900.1025.000F.*',    ;Acer
                        'PCI.1039.0900.1025.0017.*',    ;Acer
                        'PCI.1039.0900.1043.1455.*',    ;ASUS/NB
                        'PCI.1039.0900.1043.1505.*',    ;ASUS/NB
                        'PCI.1039.0900.1043.800B.*',    ;ASUS/HPD
                        'PCI.1039.0900.1043.800C.*',
                        'PCI.1039.0900.1043.8032.*',    ;ASUS 630E
                        'PCI.1039.0900.1043.8035.*',    ;ASUS 630E
                        'PCI.1039.0900.1043.8078.*',    ;ASUS 630E
                        'PCI.1039.0900.1043.807C.*',    ;ASUS 630E
                        'PCI.1039.0900.1043.80E1.*',    ;ASUS 630E
                        'PCI.1039.0900.1043.80E2.*',    ;ASUS 630E
                        'PCI.1039.0900.104D.80D5.*',    ;ASUS/SONY
                        'PCI.1039.0900.104D.FFFF.*',    ;ASUS/SONY
                        'PCI.1039.0900.1054.0900.*',    ;Hitachi
                        'PCI.1039.0900.1059.2419.*',    
                        'PCI.1039.0900.1071.7010.*',    ;Mitac/NB
                        'PCI.1039.0900.1071.7120.*',    ;Mitac/NB
                        'PCI.1039.0900.1071.7121.*',    ;Mitac/NB
                        'PCI.1039.0900.1071.7333.*',    ;Mitac/NB
                        'PCI.1039.0900.1071.7521.*',    ;Mitac
                        'PCI.1039.0900.1071.7522.*',    ;Mitac
                        'PCI.1039.0900.1071.7762.*',    ;Mitac
                        'PCI.1039.0900.1071.8640.*',    ;Mitac
                        'PCI.1039.0900.107D.0900.*',    ;Leadtek
                        'PCI.1039.0900.107D.5330.*',    ;Leadtek
                        'PCI.1039.0900.107D.5340.*',    ;Leadtek
                        'PCI.1039.0900.107D.5350.*',    ;Leadtek
                        'PCI.1039.0900.1098.630E.*',    ;QDI
                        'PCI.1039.0900.109F.7101.*',    ;Trigem
                        'PCI.1039.0900.109F.7141.*',    ;Trigem
                        'PCI.1039.0900.1170.1109.*',    ;Inventec
                        'PCI.1039.0900.1170.3209.*',    ;Inventec
                        'PCI.1039.0900.1297.0630.*',    ;Shuttle
                        'PCI.1039.0900.13BD.1016.*',    ;Mitac/NB
                        'PCI.1039.0900.13BD.101B.*',    ;Mitac/NB
                        'PCI.1039.0900.13BD.1022.*',    ;Mitac
                        'PCI.1039.0900.13BD.102C.*',    ;Mitac
                        'PCI.1039.0900.13BD.1804.*',    ;Mitac/Sharp
                        'PCI.1039.0900.1458.3100.*',    ;Gigabyte
                        'PCI.1039.0900.1458.E000.*',    ;Gigabyte
                        'PCI.1039.0900.1462.1003.*',    ;MSI
                        'PCI.1039.0900.1462.558C.*',    ;MSI
                        'PCI.1039.0900.14A4.2089.*',    ;GVC
                        'PCI.1039.0900.14A4.2097.*',    ;GVC
                        'PCI.1039.0900.14A4.2134.*',    ;GVC
                        'PCI.1039.0900.14A4.2136.*',    ;GVC
                        'PCI.1039.0900.14A4.2137.*',    ;GVC
                        'PCI.1039.0900.14A4.2153.*',    ;GVC
                        'PCI.1039.0900.14CD.2193.*',    ;USI
                        'PCI.1039.0900.14CD.2194.*',    ;USI
                        'PCI.1039.0900.14CD.21B1.*',    ;USI
                        'PCI.1039.0900.14CD.21B7.*',    ;USI
                        'PCI.1039.0900.14FF.0201.*',    ;Twinhead
                        'PCI.1039.0900.14FF.0405.*',    ;Twinhead
                        'PCI.1039.0900.14FF.0900.*',    ;Twinhead
                        'PCI.1039.0900.14FF.1100.*',    ;Twinhead
                        'PCI.1039.0900.1509.901A.*',    
                        'PCI.1039.0900.1509.901B.*',    
                        'PCI.1039.0900.1509.901C.*',    
                        'PCI.1039.0900.1509.9038.*',    
                        'PCI.1039.0900.152D.8807.*',    ;QUANTA
                        'PCI.1039.0900.1558.1103.*',    ;Clevo
                        'PCI.1039.0900.1558.1104.*',
                        'PCI.1039.0900.1558.1800.*',    ;Clevo/1800
                        'PCI.1039.0900.1558.2000.*',    ;Clevo/LP200
                        'PCI.1039.0900.1558.2200.*',    ;Clevo
                        'PCI.1039.0900.1558.2202.*',    ;Clevo/2200C/2700C
                        'PCI.1039.0900.1558.2204.*',    ;Clevo/2200S
                        'PCI.1039.0900.1558.2205.*',    ;Clevo/2200T
                        'PCI.1039.0900.1558.4201.*',    ;Clevo/2200T
                        'PCI.1039.0900.1558.5104.*',    ;Clevo/5100S
                        'PCI.1039.0900.1558.6000.*',    ;Clevo IAD-6000
                        'PCI.1039.0900.1565.0074.*',    ;Biostar
                        'PCI.1039.0900.1565.0081.*',    ;Biostar
                        'PCI.1039.0900.1565.0090.*',    ;Biostar
                        'PCI.1039.0900.1565.00F0.*',    ;Biostar
                        'PCI.1039.0900.1565.00F1.*',    ;Biostar
                        'PCI.1039.0900.156D.B500.*',    ;Alphatop
                        'PCI.1039.0900.156D.B725.*',    ;Alphatop
                        'PCI.1039.0900.156D.B901.*',    ;Alphatop
                        'PCI.1039.0900.156D.B928.*',    ;Alphatop
                        'PCI.1039.0900.1584.5001.*',    ;Uniwill
                        'PCI.1039.0900.1584.5002.*',    ;Uniwill
                        'PCI.1039.0900.1584.5003.*',    ;Uniwill
                        'PCI.1039.0900.1584.5004.*',    ;Uniwill
                        'PCI.1039.0900.1584.5005.*',    ;Uniwill
                        'PCI.1039.0900.1584.5006.*',    ;Uniwill/630
                        'PCI.1039.0900.1584.5007.*',    ;Uniwill/630
                        'PCI.1039.0900.1584.5010.*',    ;Uniwill/630
                        'PCI.1039.0900.1584.5011.*',    ;Uniwill/630
                        'PCI.1039.0900.1584.5012.*',    ;Uniwill/630
                        'PCI.1039.0900.1584.5013.*',    ;Uniwill/630
                        'PCI.1039.0900.1584.5020.*',    ;Uniwill/630
                        'PCI.1039.0900.1584.5021.*',    ;Uniwill/630
                        'PCI.1039.0900.1584.5022.*',    ;Uniwill/630
                        'PCI.1039.0900.1584.5023.*',    ;Uniwill/630
                        'PCI.1039.0900.1584.6001.*',    ;Uniwill
                        'PCI.1039.0900.1584.6002.*',    ;Uniwill
                        'PCI.1039.0900.1584.6003.*',    ;Uniwill
                        'PCI.1039.0900.1584.6004.*',    ;Uniwill
                        'PCI.1039.0900.1584.6005.*',    ;Uniwill
                        'PCI.1039.0900.15BD.1003.*',    
                        'PCI.1039.0900.15C5.0002.*',    ;Procomp
                        'PCI.1039.0900.15C5.0112.*',    ;Procomp
                        'PCI.1039.0900.15D5.3160.*',    ;Tatung
                        'PCI.1039.0900.15D5.6360.*',    ;Tatung
                        'PCI.1039.0900.15D5.7160.*',    ;Tatung
                        'PCI.1039.0900.15D5.8167.*',    ;Tatung
                        'PCI.1039.0900.15D5.8383.*',    ;Tatung
                        'PCI.1039.0900.1631.7000.*',    
                        'PCI.1039.0900.165D.0800.*',    ;PCChips
                        'PCI.1039.0900.165D.8810.*',    ;PCChips
                        'PCI.1039.0900.168F.0005.*',    
                        'PCI.1039.0900.1695.2002.*',    
                        'PCI.1039.0900.17C4.0218.*',    
                        'PCI.1039.0900.17C4.2001.*',    
                        'PCI.1039.0900.270F.A162.*',    ;ChainTech
                        'PCI.1039.0900.270F.A163.*',    ;ChainTech
                        'PCI.1039.0900.270F.A172.*',    ;ChainTech
                        'PCI.1039.0900.270F.A182.*',    ;ChainTech/Epson USI/LCDPC
                        'PCI.1039.0900.270F.A372.*',    ;ChainTech
                        'PCI.1039.0900.270F.A562.*',    ;ChainTech
                        'PCI.1039.0900.3411.0645.*',    ;QDI
                        'PCI.1039.0900.3411.0650.*',    ;QDI
                        'PCI.1039.0900.3411.630E.*',    ;QDI
                        'PCI.1039.0900.A0A0.0021.*',    ;Aopen
                        'PCI.1039.0900.A0A0.0068.*',    ;Aopen
                        'PCI.1039.0900.A0A0.0298.*',    ;Aopen
                        'PCI.1039.0900.A0A0.0299.*',    ;Aopen
                        'PCI.1039.0900.A0A0.02AE.*',    ;Aopen
                        'PCI.1039.0900.*.*.*'           ;All others

        FILE:           SIS900.LAN

   ;@#  Sprod: 'SiS~SiS900 Fast Ethernet Adapter'
   ;@#  Client: SIS900.COM, SIS900.LAN
   ;@#  Alias: SIS900.LAN

PR SLOT
        {
                DES:    $SIS7016_SLOT
                HELP:   $SIS7016_SLOTHELP

                TYP:   DEC
                VAL:    1-65535
                DEF:    UND
                OUT:    'SLOT=%s'
        }

LI PHYTYPE OPT
        {
                DES:    $SIS7016_PHY
                HELP:   $SIS7016_PHYHELP

                CD:     $SIS7016_PH_CD0
                CH:     $SIS7016_P_CD0
                CD:     $SIS7016_PH_CD1
                CH:     $SIS7016_P_CD1
                CD:     $SIS7016_PH_CD2
                CH:     $SIS7016_P_CD2
                DEF:    1
                OUT:    'PHY=%s'
        }

LI MEDIATYPE OPT
        {
                DES:    $SIS7016_MEDIA
                HELP:   $SIS7016_MEDIAHELP

                CD:     $SIS7016_MH_CD0
                CH:     $SIS7016_M_CD0
                CD:     $SIS7016_MH_CD1
                CH:     $SIS7016_M_CD1
                CD:     $SIS7016_MH_CD2
                CH:     $SIS7016_M_CD2
                CD:     $SIS7016_MH_CD3
                CH:     $SIS7016_M_CD3
                CD:     $SIS7016_MH_CD4
                CH:     $SIS7016_M_CD4
                DEF:    1
                OUT:    'MEDIATYPE=%s'
        }


PR NODE
; use all defaults
        {
        }


FR FrameSelect OPT
        {
        DES:            $SIS7016_FRAME
        HELP:           $SIS7016_FRAMEHELP
        CD:             $SIS7016_F_CD0
        CH:             $SIS7016_FH_CD0
        CD:             $SIS7016_F_CD1
        CH:             $SIS7016_FH_CD1
        CD:             $SIS7016_F_CD2
        CH:             $SIS7016_FH_CD2
        CD:             $SIS7016_F_CD3
        CH:             $SIS7016_FH_CD3
        DEF:            1,2,3,4
        }
; end Driver SIS7016

}


DLANG:  4
;English
        $SIS7016_DESC =  "SIS 900/7016 PCI Adapters NetWare ODI32 Driver"
        $SIS7016_HELP =  "The SIS PCI Fast Ethernet adapter's hardware
                configuration is performed by the PCI PlugNPlay BIOS.\n
                All other adapter options are specified in the
                Installation program or with driver keywords.\n
                You only need to specify NetWare configuration
                information or the adapter's SLOT number
                if multiple SIS PCI adapters are being used."
        $SIS7016_SLOT  = "Slot Number"
        $SIS7016_SLOTHELP = "Select the slot number"

        $SIS7016_PHY = "PHY Selection"
        $SIS7016_PHYHELP = "You can select a specific physical layer type
                to use or you can let the driver software
                automatically determine the physical layer type."
        $SIS7016_P_CD0 = "AUTO"
        $SIS7016_PH_CD0 = "Auto Detect"
        $SIS7016_P_CD1 = "LAN"
        $SIS7016_PH_CD1 = "LAN physical layer"
        $SIS7016_P_CD2 = "HOME"
        $SIS7016_PH_CD2 = "HomePNA physical layer"

        $SIS7016_MEDIA = "Media type and Speed"
        $SIS7016_MEDIAHELP = "You can select a specific media type and speed
                to use or you can let the driver software
                automatically determine the media type and speed."
        $SIS7016_M_CD0 = "AUTO"
        $SIS7016_MH_CD0 = "Auto Detect"
        $SIS7016_M_CD1 = "UTP"
        $SIS7016_MH_CD1 = "10MBPS"
        $SIS7016_M_CD2 = "UTPFULL"
        $SIS7016_MH_CD2 = "10MBPS Full Duplex"
        $SIS7016_M_CD3 = "FAST"
        $SIS7016_MH_CD3 = "100MBPS"
        $SIS7016_M_CD4 = "FASTFULL"
        $SIS7016_MH_CD4  = "100MBPS Full Duplex"

        $SIS7016_FRAME = "Ethernet Frame Type selections"
        $SIS7016_FRAMEHELP = "The driver defaults to using the 802.2
                frame type.  You can remove this frame type
                and/or add 802.3, 802.2 SNAP, or Ethernet II
                frame types. \nSelect the frame type that is used
                by the protocol that your network requires.\n
                If you select a frame type other than the default,
                configure both the server and the client to use
                the same frame type.\n
                We recommend that you select at least 802.2.\n
                For existing networks, select both 802.2 and 802.3."
        $SIS7016_F_CD0 = "802.2"
        $SIS7016_FH_CD0 = "Ethernet_802.2"
        $SIS7016_F_CD1 = "802.3"
        $SIS7016_FH_CD1 = "Ethernet_802.3"
        $SIS7016_F_CD2 = "802.2 SNAP"
        $SIS7016_FH_CD2 = "Ethernet_SNAP"
        $SIS7016_F_CD3 = "Ethernet II"
        $SIS7016_FH_CD3 = "Ethernet_II"

LANG:   6
;French
        $SIS7016_DESC =  "SIS 900/7016 PCI Adapters NetWare ODI32 Driver"
        $SIS7016_HELP =  "The SIS PCI Fast Ethernet adapter's hardware
                configuration is performed by the PCI PlugNPlay BIOS.\n
                All other adapter options are specified in the
                Installation program or with driver keywords.\n
                You only need to specify NetWare configuration
                information or the adapter's SLOT number
                if multiple SIS PCI adapters are being used."
        $SIS7016_SLOT = "Slot Number"
        $SIS7016_SLOTHELP = "Select the slot number"

        $SIS7016_PHY = "PHY Selection"
        $SIS7016_PHYHELP = "You can select a specific physical layer type
                to use or you can let the driver software
                automatically determine the physical layer type."
        $SIS7016_P_CD0 = "AUTO"
        $SIS7016_PH_CD0 = "Auto Detect"
        $SIS7016_P_CD1 = "LAN"
        $SIS7016_PH_CD1 = "LAN physical layer"
        $SIS7016_P_CD2 = "HOME"
        $SIS7016_PH_CD2 = "HomePNA physical layer"

        $SIS7016_MEDIA = "Media type and Speed"
        $SIS7016_MEDIAHELP = "You can select a specific media type and speed
                to use or you can let the driver software
                automatically determine the media type and speed."
        $SIS7016_M_CD0 = "AUTO"
        $SIS7016_MH_CD0 = "Auto Detect"
        $SIS7016_M_CD1 = "UTP"
        $SIS7016_MH_CD1 = "10MBPS"
        $SIS7016_M_CD2 = "UTPFULL"
        $SIS7016_MH_CD2 = "10MBPS Full Duplex"
        $SIS7016_M_CD3 = "FAST"
        $SIS7016_MH_CD3 = "100MBPS"
        $SIS7016_M_CD4 = "FASTFULL"
        $SIS7016_MH_CD4  = "100MBPS Full Duplex"

        $SIS7016_FRAME = "Ethernet Frame Type selections"
        $SIS7016_FRAMEHELP = "The driver defaults to using the 802.2
                frame type.  You can remove this frame type
                and/or add 802.3, 802.2 SNAP, or Ethernet II
                frame types. \nSelect the frame type that is used
                by the protocol that your network requires.\n
                If you select a frame type other than the default,
                configure both the server and the client to use
                the same frame type.\n
                We recommend that you select at least 802.2.\n
                For existing networks, select both 802.2 and 802.3."
        $SIS7016_F_CD0 = "802.2"
        $SIS7016_FH_CD0 = "Ethernet_802.2"
        $SIS7016_F_CD1 = "802.3"
        $SIS7016_FH_CD1 = "Ethernet_802.3"
        $SIS7016_F_CD2 = "802.2 SNAP"
        $SIS7016_FH_CD2 = "Ethernet_SNAP"
        $SIS7016_F_CD3 = "Ethernet II"
        $SIS7016_FH_CD3 = "Ethernet_II"

LANG:   7
;German
        $SIS7016_DESC =  "SIS 900/7016 PCI Adapters NetWare ODI32 Driver"
        $SIS7016_HELP =  "The SIS PCI Fast Ethernet adapter's hardware
                configuration is performed by the PCI PlugNPlay BIOS.\n
                All other adapter options are specified in the
                Installation program or with driver keywords.\n
                You only need to specify NetWare configuration
                information or the adapter's SLOT number
                if multiple SIS PCI adapters are being used."

        $SIS7016_SLOT = "Slot Number"
        $SIS7016_SLOTHELP = "Select the slot number"

        $SIS7016_PHY = "PHY Selection"
        $SIS7016_PHYHELP = "You can select a specific physical layer type
                to use or you can let the driver software
                automatically determine the physical layer type."
        $SIS7016_P_CD0 = "AUTO"
        $SIS7016_PH_CD0 = "Auto Detect"
        $SIS7016_P_CD1 = "LAN"
        $SIS7016_PH_CD1 = "LAN physical layer"
        $SIS7016_P_CD2 = "HOME"
        $SIS7016_PH_CD2 = "HomePNA physical layer"

        $SIS7016_MEDIA = "Media type and Speed"
        $SIS7016_MEDIAHELP = "You can select a specific media type and speed
                to use or you can let the driver software
                automatically determine the media type and speed."
        $SIS7016_M_CD0 = "AUTO"
        $SIS7016_MH_CD0 = "Auto Detect"
        $SIS7016_M_CD1 = "UTP"
        $SIS7016_MH_CD1 = "10MBPS"
        $SIS7016_M_CD2 = "UTPFULL"
        $SIS7016_MH_CD2 = "10MBPS Full Duplex"
        $SIS7016_M_CD3 = "FAST"
        $SIS7016_MH_CD3 = "100MBPS"
        $SIS7016_M_CD4 = "FASTFULL"
        $SIS7016_MH_CD4  = "100MBPS Full Duplex"

        $SIS7016_FRAME = "Ethernet Frame Type selections"
        $SIS7016_FRAMEHELP = "The driver defaults to using the 802.2
                frame type.  You can remove this frame type
                and/or add 802.3, 802.2 SNAP, or Ethernet II
                frame types. \nSelect the frame type that is used
                by the protocol that your network requires.\n
                If you select a frame type other than the default,
                configure both the server and the client to use
                the same frame type.\n
                We recommend that you select at least 802.2.\n
                For existing networks, select both 802.2 and 802.3."
        $SIS7016_F_CD0 = "802.2"
        $SIS7016_FH_CD0 = "Ethernet_802.2"
        $SIS7016_F_CD1 = "802.3"
        $SIS7016_FH_CD1 = "Ethernet_802.3"
        $SIS7016_F_CD2 = "802.2 SNAP"
        $SIS7016_FH_CD2 = "Ethernet_SNAP"
        $SIS7016_F_CD3 = "Ethernet II"
        $SIS7016_FH_CD3 = "Ethernet_II"

LANG:   8
;Italian
        $SIS7016_DESC =  "SIS 900/7016 PCI Adapters NetWare ODI32 Driver"
        $SIS7016_HELP =  "The SIS PCI Fast Ethernet adapter's hardware
                configuration is performed by the PCI PlugNPlay BIOS.\n
                All other adapter options are specified in the
                Installation program or with driver keywords.\n
                You only need to specify NetWare configuration
                information or the adapter's SLOT number
                if multiple SIS PCI adapters are being used."

        $SIS7016_SLOT = "Slot Number"
        $SIS7016_SLOTHELP = "Select the slot number"

        $SIS7016_PHY = "PHY Selection"
        $SIS7016_PHYHELP = "You can select a specific physical layer type
                to use or you can let the driver software
                automatically determine the physical layer type."
        $SIS7016_P_CD0 = "AUTO"
        $SIS7016_PH_CD0 = "Auto Detect"
        $SIS7016_P_CD1 = "LAN"
        $SIS7016_PH_CD1 = "LAN physical layer"
        $SIS7016_P_CD2 = "HOME"
        $SIS7016_PH_CD2 = "HomePNA physical layer"

        $SIS7016_MEDIA = "Media type and Speed"
        $SIS7016_MEDIAHELP = "You can select a specific media type and speed
                to use or you can let the driver software
                automatically determine the media type and speed."
        $SIS7016_M_CD0 = "AUTO"
        $SIS7016_MH_CD0 = "Auto Detect"
        $SIS7016_M_CD1 = "UTP"
        $SIS7016_MH_CD1 = "10MBPS"
        $SIS7016_M_CD2 = "UTPFULL"
        $SIS7016_MH_CD2 = "10MBPS Full Duplex"
        $SIS7016_M_CD3 = "FAST"
        $SIS7016_MH_CD3 = "100MBPS"
        $SIS7016_M_CD4 = "FASTFULL"
        $SIS7016_MH_CD4  = "100MBPS Full Duplex"

        $SIS7016_FRAME = "Ethernet Frame Type selections"
        $SIS7016_FRAMEHELP = "The driver defaults to using the 802.2
                frame type.  You can remove this frame type
                and/or add 802.3, 802.2 SNAP, or Ethernet II
                frame types. \nSelect the frame type that is used
                by the protocol that your network requires.\n
                If you select a frame type other than the default,
                configure both the server and the client to use
                the same frame type.\n
                We recommend that you select at least 802.2.\n
                For existing networks, select both 802.2 and 802.3."
        $SIS7016_F_CD0 = "802.2"
        $SIS7016_FH_CD0 = "Ethernet_802.2"
        $SIS7016_F_CD1 = "802.3"
        $SIS7016_FH_CD1 = "Ethernet_802.3"
        $SIS7016_F_CD2 = "802.2 SNAP"
        $SIS7016_FH_CD2 = "Ethernet_SNAP"
        $SIS7016_F_CD3 = "Ethernet II"
        $SIS7016_FH_CD3 = "Ethernet_II"

LANG:   14
;Spanish
        $SIS7016_DESC =  "SIS 900/7016 PCI Adapters NetWare ODI32 Driver"
        $SIS7016_HELP =  "The SIS PCI Fast Ethernet adapter's hardware
                configuration is performed by the PCI PlugNPlay BIOS.\n
                All other adapter options are specified in the
                Installation program or with driver keywords.\n
                You only need to specify NetWare configuration
                information or the adapter's SLOT number
                if multiple SIS PCI adapters are being used."

        $SIS7016_SLOT = "Slot Number"
        $SIS7016_SLOTHELP = "Select the slot number"

        $SIS7016_PHY = "PHY Selection"
        $SIS7016_PHYHELP = "You can select a specific physical layer type
                to use or you can let the driver software
                automatically determine the physical layer type."
        $SIS7016_P_CD0 = "AUTO"
        $SIS7016_PH_CD0 = "Auto Detect"
        $SIS7016_P_CD1 = "LAN"
        $SIS7016_PH_CD1 = "LAN physical layer"
        $SIS7016_P_CD2 = "HOME"
        $SIS7016_PH_CD2 = "HomePNA physical layer"

        $SIS7016_MEDIA = "Media type and Speed"
        $SIS7016_MEDIAHELP = "You can select a specific media type and speed
                to use or you can let the driver software
                automatically determine the media type and speed."
        $SIS7016_M_CD0 = "AUTO"
        $SIS7016_MH_CD0 = "Auto Detect"
        $SIS7016_M_CD1 = "UTP"
        $SIS7016_MH_CD1 = "10MBPS"
        $SIS7016_M_CD2 = "UTPFULL"
        $SIS7016_MH_CD2 = "10MBPS Full Duplex"
        $SIS7016_M_CD3 = "FAST"
        $SIS7016_MH_CD3 = "100MBPS"
        $SIS7016_M_CD4 = "FASTFULL"
        $SIS7016_MH_CD4  = "100MBPS Full Duplex"

        $SIS7016_FRAME = "Ethernet Frame Type selections"
        $SIS7016_FRAMEHELP = "The driver defaults to using the 802.2
                frame type.  You can remove this frame type
                and/or add 802.3, 802.2 SNAP, or Ethernet II
                frame types. \nSelect the frame type that is used
                by the protocol that your network requires.\n
                If you select a frame type other than the default,
                configure both the server and the client to use
                the same frame type.\n
                We recommend that you select at least 802.2.\n
                For existing networks, select both 802.2 and 802.3."
        $SIS7016_F_CD0 = "802.2"
        $SIS7016_FH_CD0 = "Ethernet_802.2"
        $SIS7016_F_CD1 = "802.3"
        $SIS7016_FH_CD1 = "Ethernet_802.3"
        $SIS7016_F_CD2 = "802.2 SNAP"
        $SIS7016_FH_CD2 = "Ethernet_SNAP"
        $SIS7016_F_CD3 = "Ethernet II"
        $SIS7016_FH_CD3 = "Ethernet_II"

LANG:   12
;Portugese
        $SIS7016_DESC =  "SIS 900/7016 PCI Adapters NetWare ODI32 Driver"
        $SIS7016_HELP =  "The SIS PCI Fast Ethernet adapter's hardware
                configuration is performed by the PCI PlugNPlay BIOS.\n
                All other adapter options are specified in the
                Installation program or with driver keywords.\n
                You only need to specify NetWare configuration
                information or the adapter's SLOT number
                if multiple SIS PCI adapters are being used."

        $SIS7016_SLOT = "Slot Number"
        $SIS7016_SLOTHELP = "Select the slot number"

        $SIS7016_PHY = "PHY Selection"
        $SIS7016_PHYHELP = "You can select a specific physical layer type
                to use or you can let the driver software
                automatically determine the physical layer type."
        $SIS7016_P_CD0 = "AUTO"
        $SIS7016_PH_CD0 = "Auto Detect"
        $SIS7016_P_CD1 = "LAN"
        $SIS7016_PH_CD1 = "LAN physical layer"
        $SIS7016_P_CD2 = "HOME"
        $SIS7016_PH_CD2 = "HomePNA physical layer"

        $SIS7016_MEDIA = "Media type and Speed"
        $SIS7016_MEDIAHELP = "You can select a specific media type and speed
                to use or you can let the driver software
                automatically determine the media type and speed."
        $SIS7016_M_CD0 = "AUTO"
        $SIS7016_MH_CD0 = "Auto Detect"
        $SIS7016_M_CD1 = "UTP"
        $SIS7016_MH_CD1 = "10MBPS"
        $SIS7016_M_CD2 = "UTPFULL"
        $SIS7016_MH_CD2 = "10MBPS Full Duplex"
        $SIS7016_M_CD3 = "FAST"
        $SIS7016_MH_CD3 = "100MBPS"
        $SIS7016_M_CD4 = "FASTFULL"
        $SIS7016_MH_CD4  = "100MBPS Full Duplex"

        $SIS7016_FRAME = "Ethernet Frame Type selections"
        $SIS7016_FRAMEHELP = "The driver defaults to using the 802.2
                frame type.  You can remove this frame type
                and/or add 802.3, 802.2 SNAP, or Ethernet II
                frame types. \nSelect the frame type that is used
                by the protocol that your network requires.\n
                If you select a frame type other than the default,
                configure both the server and the client to use
                the same frame type.\n
                We recommend that you select at least 802.2.\n
                For existing networks, select both 802.2 and 802.3."
        $SIS7016_F_CD0 = "802.2"
        $SIS7016_FH_CD0 = "Ethernet_802.2"
        $SIS7016_F_CD1 = "802.3"
        $SIS7016_FH_CD1 = "Ethernet_802.3"
        $SIS7016_F_CD2 = "802.2 SNAP"
        $SIS7016_FH_CD2 = "Ethernet_SNAP"
        $SIS7016_F_CD3 = "Ethernet II"
        $SIS7016_FH_CD3 = "Ethernet_II"

LANG:   9
;Japanese
        $SIS7016_DESC =  "SIS 900/7016 PCI Adapters NetWare ODI32 Driver"
        $SIS7016_HELP =  "The SIS PCI Fast Ethernet adapter's hardware
                configuration is performed by the PCI PlugNPlay BIOS.\n
                All other adapter options are specified in the
                Installation program or with driver keywords.\n
                You only need to specify NetWare configuration
                information or the adapter's SLOT number
                if multiple SIS PCI adapters are being used."

        $SIS7016_SLOT = "Slot Number"
        $SIS7016_SLOTHELP = "Select the slot number"

        $SIS7016_PHY = "PHY Selection"
        $SIS7016_PHYHELP = "You can select a specific physical layer type
                to use or you can let the driver software
                automatically determine the physical layer type."
        $SIS7016_P_CD0 = "AUTO"
        $SIS7016_PH_CD0 = "Auto Detect"
        $SIS7016_P_CD1 = "LAN"
        $SIS7016_PH_CD1 = "LAN physical layer"
        $SIS7016_P_CD2 = "HOME"
        $SIS7016_PH_CD2 = "HomePNA physical layer"

        $SIS7016_MEDIA = "Media type and Speed"
        $SIS7016_MEDIAHELP = "You can select a specific media type and speed
                to use or you can let the driver software
                automatically determine the media type and speed."
        $SIS7016_M_CD0 = "AUTO"
        $SIS7016_MH_CD0 = "Auto Detect"
        $SIS7016_M_CD1 = "UTP"
        $SIS7016_MH_CD1 = "10MBPS"
        $SIS7016_M_CD2 = "UTPFULL"
        $SIS7016_MH_CD2 = "10MBPS Full Duplex"
        $SIS7016_M_CD3 = "FAST"
        $SIS7016_MH_CD3 = "100MBPS"
        $SIS7016_M_CD4 = "FASTFULL"
        $SIS7016_MH_CD4  = "100MBPS Full Duplex"

        $SIS7016_FRAME = "Ethernet Frame Type selections"
        $SIS7016_FRAMEHELP = "The driver defaults to using the 802.2
                frame type.  You can remove this frame type
                and/or add 802.3, 802.2 SNAP, or Ethernet II
                frame types. \nSelect the frame type that is used
                by the protocol that your network requires.\n
                If you select a frame type other than the default,
                configure both the server and the client to use
                the same frame type.\n
                We recommend that you select at least 802.2.\n
                For existing networks, select both 802.2 and 802.3."
        $SIS7016_F_CD0 = "802.2"
        $SIS7016_FH_CD0 = "Ethernet_802.2"
        $SIS7016_F_CD1 = "802.3"
        $SIS7016_FH_CD1 = "Ethernet_802.3"
        $SIS7016_F_CD2 = "802.2 SNAP"
        $SIS7016_FH_CD2 = "Ethernet_SNAP"
        $SIS7016_F_CD3 = "Ethernet II"
        $SIS7016_FH_CD3 = "Ethernet_II"

LANG:   10
;Korean
        $SIS7016_DESC =  "SIS 900/7016 PCI Adapters NetWare ODI32 Driver"
        $SIS7016_HELP =  "The SIS PCI Fast Ethernet adapter's hardware
                configuration is performed by the PCI PlugNPlay BIOS.\n
                All other adapter options are specified in the
                Installation program or with driver keywords.\n
                You only need to specify NetWare configuration
                information or the adapter's SLOT number
                if multiple SIS PCI adapters are being used."

        $SIS7016_SLOT = "Slot Number"
        $SIS7016_SLOTHELP = "Select the slot number"

        $SIS7016_PHY = "PHY Selection"
        $SIS7016_PHYHELP = "You can select a specific physical layer type
                to use or you can let the driver software
                automatically determine the physical layer type."
        $SIS7016_P_CD0 = "AUTO"
        $SIS7016_PH_CD0 = "Auto Detect"
        $SIS7016_P_CD1 = "LAN"
        $SIS7016_PH_CD1 = "LAN physical layer"
        $SIS7016_P_CD2 = "HOME"
        $SIS7016_PH_CD2 = "HomePNA physical layer"

        $SIS7016_MEDIA = "Media type and Speed"
        $SIS7016_MEDIAHELP = "You can select a specific media type and speed
                to use or you can let the driver software
                automatically determine the media type and speed."
        $SIS7016_M_CD0 = "AUTO"
        $SIS7016_MH_CD0 = "Auto Detect"
        $SIS7016_M_CD1 = "UTP"
        $SIS7016_MH_CD1 = "10MBPS"
        $SIS7016_M_CD2 = "UTPFULL"
        $SIS7016_MH_CD2 = "10MBPS Full Duplex"
        $SIS7016_M_CD3 = "FAST"
        $SIS7016_MH_CD3 = "100MBPS"
        $SIS7016_M_CD4 = "FASTFULL"
        $SIS7016_MH_CD4  = "100MBPS Full Duplex"

        $SIS7016_FRAME = "Ethernet Frame Type selections"
        $SIS7016_FRAMEHELP = "The driver defaults to using the 802.2
                frame type.  You can remove this frame type
                and/or add 802.3, 802.2 SNAP, or Ethernet II
                frame types. \nSelect the frame type that is used
                by the protocol that your network requires.\n
                If you select a frame type other than the default,
                configure both the server and the client to use
                the same frame type.\n
                We recommend that you select at least 802.2.\n
                For existing networks, select both 802.2 and 802.3."
        $SIS7016_F_CD0 = "802.2"
        $SIS7016_FH_CD0 = "Ethernet_802.2"
        $SIS7016_F_CD1 = "802.3"
        $SIS7016_FH_CD1 = "Ethernet_802.3"
        $SIS7016_F_CD2 = "802.2 SNAP"
        $SIS7016_FH_CD2 = "Ethernet_SNAP"
        $SIS7016_F_CD3 = "Ethernet II"
        $SIS7016_FH_CD3 = "Ethernet_II"

LANG:   1
;Chinese-Simplified
        $SIS7016_DESC =  "SIS 900/7016 PCI Adapters NetWare ODI32 Driver"
        $SIS7016_HELP =  "The SIS PCI Fast Ethernet adapter's hardware
                configuration is performed by the PCI PlugNPlay BIOS.\n
                All other adapter options are specified in the
                Installation program or with driver keywords.\n
                You only need to specify NetWare configuration
                information or the adapter's SLOT number
                if multiple SIS PCI adapters are being used."

        $SIS7016_SLOT = "Slot Number"
        $SIS7016_SLOTHELP = "Select the slot number"

        $SIS7016_PHY = "PHY Selection"
        $SIS7016_PHYHELP = "You can select a specific physical layer type
                to use or you can let the driver software
                automatically determine the physical layer type."
        $SIS7016_P_CD0 = "AUTO"
        $SIS7016_PH_CD0 = "Auto Detect"
        $SIS7016_P_CD1 = "LAN"
        $SIS7016_PH_CD1 = "LAN physical layer"
        $SIS7016_P_CD2 = "HOME"
        $SIS7016_PH_CD2 = "HomePNA physical layer"

        $SIS7016_MEDIA = "Media type and Speed"
        $SIS7016_MEDIAHELP = "You can select a specific media type and speed
                to use or you can let the driver software
                automatically determine the media type and speed."
        $SIS7016_M_CD0 = "AUTO"
        $SIS7016_MH_CD0 = "Auto Detect"
        $SIS7016_M_CD1 = "UTP"
        $SIS7016_MH_CD1 = "10MBPS"
        $SIS7016_M_CD2 = "UTPFULL"
        $SIS7016_MH_CD2 = "10MBPS Full Duplex"
        $SIS7016_M_CD3 = "FAST"
        $SIS7016_MH_CD3 = "100MBPS"
        $SIS7016_M_CD4 = "FASTFULL"
        $SIS7016_MH_CD4  = "100MBPS Full Duplex"

        $SIS7016_FRAME = "Ethernet Frame Type selections"
        $SIS7016_FRAMEHELP = "The driver defaults to using the 802.2
                frame type.  You can remove this frame type
                and/or add 802.3, 802.2 SNAP, or Ethernet II
                frame types. \nSelect the frame type that is used
                by the protocol that your network requires.\n
                If you select a frame type other than the default,
                configure both the server and the client to use
                the same frame type.\n
                We recommend that you select at least 802.2.\n
                For existing networks, select both 802.2 and 802.3."
        $SIS7016_F_CD0 = "802.2"
        $SIS7016_FH_CD0 = "Ethernet_802.2"
        $SIS7016_F_CD1 = "802.3"
        $SIS7016_FH_CD1 = "Ethernet_802.3"
        $SIS7016_F_CD2 = "802.2 SNAP"
        $SIS7016_FH_CD2 = "Ethernet_SNAP"
        $SIS7016_F_CD3 = "Ethernet II"
        $SIS7016_FH_CD3 = "Ethernet_II"

LANG:   13
;Russian
        $SIS7016_DESC =  "SIS 900/7016 PCI Adapters NetWare ODI32 Driver"
        $SIS7016_HELP =  "The SIS PCI Fast Ethernet adapter's hardware
                configuration is performed by the PCI PlugNPlay BIOS.\n
                All other adapter options are specified in the
                Installation program or with driver keywords.\n
                You only need to specify NetWare configuration
                information or the adapter's SLOT number
                if multiple SIS PCI adapters are being used."

        $SIS7016_SLOT = "Slot Number"
        $SIS7016_SLOTHELP = "Select the slot number"

        $SIS7016_PHY = "PHY Selection"
        $SIS7016_PHYHELP = "You can select a specific physical layer type
                to use or you can let the driver software
                automatically determine the physical layer type."
        $SIS7016_P_CD0 = "AUTO"
        $SIS7016_PH_CD0 = "Auto Detect"
        $SIS7016_P_CD1 = "LAN"
        $SIS7016_PH_CD1 = "LAN physical layer"
        $SIS7016_P_CD2 = "HOME"
        $SIS7016_PH_CD2 = "HomePNA physical layer"

        $SIS7016_MEDIA = "Media type and Speed"
        $SIS7016_MEDIAHELP = "You can select a specific media type and speed
                to use or you can let the driver software
                automatically determine the media type and speed."
        $SIS7016_M_CD0 = "AUTO"
        $SIS7016_MH_CD0 = "Auto Detect"
        $SIS7016_M_CD1 = "UTP"
        $SIS7016_MH_CD1 = "10MBPS"
        $SIS7016_M_CD2 = "UTPFULL"
        $SIS7016_MH_CD2 = "10MBPS Full Duplex"
        $SIS7016_M_CD3 = "FAST"
        $SIS7016_MH_CD3 = "100MBPS"
        $SIS7016_M_CD4 = "FASTFULL"
        $SIS7016_MH_CD4  = "100MBPS Full Duplex"

        $SIS7016_FRAME = "Ethernet Frame Type selections"
        $SIS7016_FRAMEHELP = "The driver defaults to using the 802.2
                frame type.  You can remove this frame type
                and/or add 802.3, 802.2 SNAP, or Ethernet II
                frame types. \nSelect the frame type that is used
                by the protocol that your network requires.\n
                If you select a frame type other than the default,
                configure both the server and the client to use
                the same frame type.\n
                We recommend that you select at least 802.2.\n
                For existing networks, select both 802.2 and 802.3."
        $SIS7016_F_CD0 = "802.2"
        $SIS7016_FH_CD0 = "Ethernet_802.2"
        $SIS7016_F_CD1 = "802.3"
        $SIS7016_FH_CD1 = "Ethernet_802.3"
        $SIS7016_F_CD2 = "802.2 SNAP"
        $SIS7016_FH_CD2 = "Ethernet_SNAP"
        $SIS7016_F_CD3 = "Ethernet II"
        $SIS7016_FH_CD3 = "Ethernet_II"
