;*******************************************************************************
; Copyright(C) 2002
; 802.11a/g Wireless LAN Network Adapter
;
; Supported OS: Windows 98/ME/2000/XP
; 
;*******************************************************************************

[Version]
 DriverVer = 12/19/2003, 3.00.3.0
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
 CatalogFile         = MSI68NIC.cat
 MillenniumPreferred = .ME

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = *

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]
 %A001_DESC_STR%     = PRISM_A001,        PCI\VEN_1260&DEV_3890&SUBSYS_68181462
 %A002_DESC_STR%     = PRISM_A002,        PCI\VEN_1260&DEV_3886&SUBSYS_68421462
 %A003_DESC_STR%     = PRISM_A003,        PCI\VEN_1260&DEV_3886&SUBSYS_68431462
 %A004_DESC_STR%     = PRISM_A004,        PCI\VEN_1260&DEV_3886&SUBSYS_68451462
 

;==========================================
[PRISM_A001]       ; Win9x
 AddReg         = PRISM_A001.reg, COMMON_A00.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_NDI.copy

[PRISM_A001.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_A001.reg, COMMON_A00.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_NDI.copy.ME

[PRISM_A001.NT]    ; Win2k
 AddReg         = PRISM_A001.reg, COMMON_A00.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_A001.NT.Services]
 AddService     = "PRISM_A00", 2, PRISM_DRIVER_A00.Service, PRISM_DRIVER.EventLog

[PRISM_A001.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_68181462"
; 0x3890 = 14480
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%A001_DESC_STR%

;==========================================
[PRISM_A002]       ; Win9x
 AddReg         = PRISM_A002.reg, COMMON_A00.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_NDI.copy

[PRISM_A002.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_A002.reg, COMMON_A00.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_NDI.copy.ME

[PRISM_A002.NT]    ; Win2k
 AddReg         = PRISM_A002.reg, COMMON_A00.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_A002.NT.Services]
 AddService     = "PRISM_A00", 2, PRISM_DRIVER_A00.Service, PRISM_DRIVER.EventLog

[PRISM_A002.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3886&SUBSYS_68421462"
; 0x3886 = 14470, but same functions as 3890
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%A002_DESC_STR%

;==========================================
[PRISM_A003]       ; Win9x
 AddReg         = PRISM_A003.reg, COMMON_A00.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_NDI.copy

[PRISM_A003.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_A003.reg, COMMON_A00.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_NDI.copy.ME

[PRISM_A003.NT]    ; Win2k
 AddReg         = PRISM_A003.reg, COMMON_A00.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_A003.NT.Services]
 AddService     = "PRISM_A00", 2, PRISM_DRIVER_A00.Service, PRISM_DRIVER.EventLog

[PRISM_A003.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3886&SUBSYS_68431462"
; 0x3886 = 14470, but same functions as 3890
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%A003_DESC_STR%

;==========================================
[PRISM_A004]       ; Win9x
 AddReg         = PRISM_A004.reg, COMMON_A00.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_NDI.copy

[PRISM_A004.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_A004.reg, COMMON_A00.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_NDI.copy.ME

[PRISM_A004.NT]    ; Win2k
 AddReg         = PRISM_A004.reg, COMMON_A00.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_A004.NT.Services]
 AddService     = "PRISM_A00", 2, PRISM_DRIVER_A00.Service, PRISM_DRIVER.EventLog

[PRISM_A004.reg]
 HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3886&SUBSYS_68451462"
; 0x3886 = 14470, but same functions as 3890
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%A004_DESC_STR%
;###############################################################################

[PRISM_DRIVER_A00.Service]
 DisplayName    = %A00_SERVICE_STR%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\MSI68ICB.sys
 LoadOrderGroup = NDIS

[PRISM_DRIVER.EventLog]
 AddReg         = PRISM_DRIVER.EventLog.reg

[PRISM_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################

[COMMON_A00.reg]
 HKR,NDI                ,Service                    ,0  ,"PRISM_A00"
 HKR,                   ,BusType                    ,0  ,"5"
 HKR,                   ,DeviceVxDs                 ,0  ,"MSI68ICB.sys"
 HKR,                   ,CardBusBridgeLatencyTimer  ,0  ,"32"
 HKR,                   ,CardBusBridgeCacheLineSize ,0  ,"8"

[COMMON_NDIS.reg]
; Win9X
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,NDI                ,NdiInstaller           ,0      ,"PRISMNDI.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.ME]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,NDI                ,NdiInstaller           ,0      ,"PRISMNDI.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.NT]
 HKR,                   ,EnumPropPages32        ,0      ,"PRISMNDI.dll,NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

[COMMON.reg]
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,,RTSThresh,0,2347
 HKR,Ndi\params\RTSThresh,default,0,2347
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2347
 HKR,NDI\params\RTSThresh,step,0,1
 HKR,NDI\params\RTSThresh,optional,0,1

 HKR,,FragThresh,0,2346
 HKR,Ndi\params\FragThresh,default,0,2346
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2346
 HKR,NDI\params\FragThresh,step,0,2
 HKR,NDI\params\FragThresh,optional,0,1

 HKR,,ShortRetryLimit,0,7
 HKR,NDI\params\ShortRetryLimit,default,0,7
 HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
 HKR,NDI\params\ShortRetryLimit,type,,int
 HKR,NDI\params\ShortRetryLimit,min,0,1
 HKR,NDI\params\ShortRetryLimit,max,0,255
 HKR,NDI\params\ShortRetryLimit,step,0,1
 HKR,NDI\params\ShortRetryLimit,optional,0,1

 HKR,,LongRetryLimit,0,4
 HKR,NDI\params\LongRetryLimit,default,0,4
 HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
 HKR,NDI\params\LongRetryLimit,type,0,int
 HKR,NDI\params\LongRetryLimit,min,0,1
 HKR,NDI\params\LongRetryLimit,max,0,255
 HKR,NDI\params\LongRetryLimit,step,0,1
 HKR,NDI\params\LongRetryLimit,optional,0,1

 HKR,,ConfigProfile,0,3
 HKR,NDI\params\ConfigProfile,default,0,3
 HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
 HKR,NDI\params\ConfigProfile,type,,enum
 HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
 HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
 HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
 HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
 HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
 HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
 HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
 HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
 HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
 HKR,NDI\params\ConfigProfile,optional,0,1

 HKR,,NitroMode,0,"1"
 HKR,NDI\params\NitroMode,default,0,1
 HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
 HKR,NDI\params\NitroMode,type,,enum
 HKR,NDI\params\NitroMode,flag,1,30,00,00,00
 HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
 HKR,NDI\params\NitroMode\enum,1,,%ON_STR%
 HKR,NDI\params\NitroMode,optional,0,1

 HKR,,PSMode,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
 HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
 HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
 HKR,NDI\params\PSMode,optional,0,1
 
;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 PRISM_DRIVER.copy      = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.ME   = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.NT   = 12 ; Win2k=%windir%\system32\drivers

[PRISM_NDI.copy]
;PRISMNDI.dll,,,2
;PRISMAPI.dll,,,2

[PRISM_NDI.copy.ME]
 PRISMNDI.dll,,,18
;PRISMAPI.dll,,,18

[PRISM_DRIVER.copy]
;;;;
;;;;
 MSI68ICB.sys,,,2
 MSI68IOC.vxd,,,2           ; Win9x Ioctl interface

[PRISM_DRIVER.copy.ME]
;;;;
;;;;
 MSI68ICB.sys,,,18
 MSI68IOC.vxd,,,18           ; Win9x Ioctl interface

[PRISM_DRIVER.copy.NT]
;;;;
;;;;
 MSI68ICB.sys

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
; 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
 MSI68IOC.vxd           = 1,win9x
 PRISMNDI.dll           = 1,win9x
;;;;           = 1,winnt ; Install NDIS4 driver on OSR2
;;;;           = 1
 MSI68ICB.sys           = 1

[SourceDisksFiles.ME]   ; WinMe
 MSI68IOC.vxd           = 1,win9x
 PRISMNDI.dll           = 1,win9x
;;;;           = 1
;;;;           = 1
 MSI68ICB.sys           = 1

[SourceDisksFiles.X86]  ; Win2k/Xp
;;;;           = 1,winxp
;;;;           = 1,winxp
 MSI68ICB.sys           = 1

;###############################################################################
[Strings]
;String ID              = String Text
;---------                -----------
 VER_VENDOR_STR         = "802.11 Wireless"
 VER_VENDOR_NAME_STR    = "802.11 Wireless"
 INSTALL_DISK_STR       = "IEEE 802.11 Wireless Network Install Disk"

 A001_DESC_STR		= "IEEE 802.11g MiniPCI Wireless Network Adapter"
 A002_DESC_STR		= "802.11a/g CardBus Wireless Network Adapter"
 A003_DESC_STR		= "802.11a/g MiniPCI Wireless Network Adapter"
 A004_DESC_STR		= "802.11a/g PCI Wireless Network Adapter"
 A00_SERVICE_STR        = "IEEE 802.11 Driver"
 
 ON_STR                  = "On"
 OFF_STR                 = "Off"
 RTSTHRESH_STR           = "RTS Threshold"
 FRAGTHRESH_STR          = "Fragmentation Threshold"
 AUTHENT_TYPE_STR        = "Authentication Algorithm"
 POWER_SAVE_STR          = "Power Save Mode"
 POWER_SAVE_OFF_STR      = "Disabled"
 POWER_SAVE_DYN_STR      = "Dynamic"
 POWER_SAVE_MAX_STR      = "Maximum"
 SHORT_RETRY_STR         = "Short Retry Limit"
 LONG_RETRY_STR          = "Long Retry Limit"
 CONFIG_PROFILE          = "Configuration Profile"
 CONFIG_PROF_B_ONLY      = "B only"
 CONFIG_PROF_MIXED       = "Mixed"
 CONFIG_PROF_MIXED_LONG  = "Mixed Long"
 CONFIG_PROF_G_ONLY      = "G only"
 CONFIG_PROF_TEST        = "Test"
 CONFIG_PROF_B_WIFI      = "B WiFi"
 CONFIG_PROF_MIXED_SHORT = "Mixed Short"
 CONFIG_PROF_WIFI_SPEC   = "WiFi Spec"
 NITRO_MODE              = "Nitro Mode"


